For 1990-2009 cars

### Removal Procedure

1. Remove the right side console lower extension. Refer to Instrument Panel Extension Replacement.
2. Remove the instrument panel lower right trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Right Side.
3. Remove right side floor duct. Refer to Floor Air Outlet Duct Replacement - Right Side .
4. Disconnect the face/floor actuator electrical connector (3).
5. Remove the face/floor actuator to HVAC module assembly retaining screws (1).

Important: Pivot the face/floor mode actuator (3) upwards and remove the face/floor mode actuator lever (2) from the face door mode lever (1).

6. Remove the face/floor mode actuator lever (2) from the face door mode lever (1).
7. Record where the face/floor mode actuator lever (1) is located onto the face/floor actuator drive spline (2) for installation.

### Installation Procedure

1. Detach and move the face/floor mode actuator lever (1) to the recorded position on the face/floor actuator drive spline (2) as required.
2. Install the actuator lever (2) to the face door mode lever (1) and pivot the face/floor mode actuator (3) into position on the HVAC module assembly (4).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the face/floor mode actuator to HVAC module assembly retaining screws (1).

Tighten
Tighten the bolts to 1.2 N·m (9 lb ft).

4. Connect the face/floor mode actuator electrical connector (3).
5. Install the instrument panel lower right trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Right Side.
6. Install right side floor duct. Refer to Floor Air Outlet Duct Replacement - Right Side.
7. Perform HVAC system relearn. Refer to HVAC Control Module Programming and Setup.