For 1990-2009 cars

### Tools Required

KM-906-B Control Arm Bushing Remover/Installer.

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the Y-Link. Refer to Trailing Arm Replacement.

Important: It is recommended to observe the orientation and depth of the Y-Link bushing (2) with reference to the original position. Adhering to this recommendation will minimize the potential of incorrect Y-Link bushing (2) installation.

3. Remove the Y-Link bushing (2) from the Y-Link (3) using the KM-906-B (1, 4).
4. Inspect all parts for wear and damage.

### Installation Procedure

Important: Before installing, the Y-Link bushing (2) must be correctly aligned and orientated.

1. Install the Y-Link (2) bushing to the Y-Link (3) using the KM-906-B 9 (1, 4).
2. Install the Y-Link (3). Refer to Trailing Arm Replacement.
3. Remove the safety stands.
4. Lower the vehicle to the ground.