For 1990-2009 cars

## Radiator Grille Replacement LWB

### Removal Procedure

1. Remove the radiator grille to hood retaining bolts (1).
2. Carefully pry the radiator grille (2) from the hood (2).
3. Remove the radiator grille from the hood.

### Installation Procedure

1. Install the radiator grille to the front bumper fascia.
2. Firmly press the radiator grille retaining tabs (2) into the hood (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the radiator grille to hood retaining nuts (1).

Tighten
Tighten the nuts to 4 N·m (35 lb in).