For 1990-2009 cars

Checks | Action
--- | ---
DEFINITION: Knocking or clunking noise occurs when operating the vehicle in high gear or coasting in neutral at 16 km/h (10 mph).
The universal joint is worn or damaged. | Replace the complete propeller shaft. Refer to Propeller Shaft Replacement .
The rubber coupling is damaged. | Replace the rubber coupling. Refer to Rear Propeller Shaft Coupling Replacement .
The rubber coupling to propeller shaft retaining bolts and nuts are loose. | Tighten the bolts to specifications. Refer to Fastener Tightening Specifications .
The rubber coupling is damaged. | Replace the rubber coupling. Refer to Rear Propeller Shaft Coupling Replacement .
The center bearing is damaged. | Replace the center bearing. Refer to Propeller Shaft Center Support Bearing Replacement .
The side gear in the differential is worn or oversize. | Replace the differential case and/or the side gears. Refer to Differential Replacement .