For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the radiator air baffle and deflector. Refer to Front Air Deflector Replacement .
3. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
4. Remove the front energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement .
5. Remove the washer solvent container. Refer to Windshield Washer Solvent Container Replacement .
6. Remove the ambient temperature sensor (1) by squeezing locking tabs and pushing sensor.
7. Remove the front bumper impact bar to front end module retaining bolt (1). Repeat for opposite side.
8. Remove the front bumper impact bar to front end module retaining bolts (1).
9. Remove the front bumper impact bar from the front end module.

### Installation Procedure

1. Install the front bumper impact bar to the front end module.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front bumper impact bar to front end module retaining bolts (1).

2.1. | Install the inboard bolt on the right side first.

2.2. | Install the inboard bolt on the left side second.

2.3. | Install the remaining outboard bolts third.

Tighten
Tighten the bolts to 22 N·m (16 lb ft) in the above sequence.

3. Install the front bumper impact bar to front end module retaining bolt (1). Repeat for opposite side.

Tighten
Tighten the bolts to 4 N·m (35 lb in).

4. Install the ambient temperature sensor (1) by squeezing locking tabs and pushing sensor.
5. Remove the washer solvent container. Refer to Windshield Washer Solvent Container Filler Tube Replacement .
6. Install the front energy absorber. Refer to Front Bumper Fascia Energy Absorber Replacement .
7. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .
8. Install the radiator air baffle and deflector. Refer to Front Air Deflector Replacement .
9. Lower the vehicle.