For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the window inner belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
3. Remove the door garnish molding. Refer to Front and Rear Side Door Window Garnish Molding Replacement .

Important: Pry out the window inner sealing strip (1) then pull by hand to expose the door applique retaining screws.

4. Detach the front part of the window inner sealing strip (1) from the door (2).
5. Remove the door applique to door retaining screws (1).
6. Remove the door applique (1) from the door (2).

### Installation Procedure

1. Position the door applique (1) to the door (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door applique to door retaining screws (1).

Tighten
Tighten the screws to 3 N-m (27 lb in).

3. Attach the attach part of the window inner sealing strip (1) to the door (2).
4. Install the door garnish molding.Refer to Front and Rear Side Door Window Garnish Molding Replacement .
5. Install the window inner belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
6. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .