For 1990-2009 cars

## Repeater Lamp Replacement LWB

### Removal Procedure - Side Indicator Type B

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle to a suitable working height. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
3. Unclip the side indicator (2) retaining clips (1) and detach from the fender.
4. Disconnect the side indicator lamp (2) electrical connector (1).
5. Remove the side indicator lamp (2).

### Installation Procedure

1. Connect the side indicator lamp (2) electrical connector (1).
2. Align the side indicator lamp (2) with the fender.
3. Install the side indicator lamp (2) into the fender, ensuring that the retaining clips (1) are fully located in the fender. Listen for an audible click to confirm fitting.
4. Install the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
5. Lower the vehicle.
6. Test the side indicator lamp for correct operation.