For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Check Link to Door Retaining Nuts | 6 N·m | 53 lb in
Door Check Link to Pillar Retaining Bolt | 25 N·m | 18 lb ft
Door Hinge Keeper Bolt | 3 N·m | 27 lb in
Door Hinge to Door Retaining Bolts | 28 N·m | 21 lb ft
Door Hinge to Pillar Retaining Bolts | 28 N·m | 21 lb ft
Fuel Tank Filler Door to Rear Quarter Panel Retaining Screws | 2 N·m | 18 lb in
Front Fender to Body Side Retaining Bolts | 9 N·m | 80 lb in
Front Fender to Door Pillar Retaining Bolts | 9 N·m | 80 lb in
Front Fender to Front End Module Retaining Bolt | 9 N·m | 80 lb in
Front Fender to Inner Wheelhouse Retaining Bolts | 9 N·m | 80 lb in
Hood Assist Rod Upper Ball Stud | 18 N·m | 13 lb ft
Hood Hinge to Dash And Cowl Panel Brace Retaining Bolt | 20 N·m | 15 lb ft
Hood Latch to Front End Module Retaining Bolts | 9 N·m | 80 lb in
Hood Hinge to Hood Retaining Bolts | 20 N·m | 15 lb ft