For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the seat back assembly. Refer to Rear Seat Back Replacement.
3. Remove the rear sill trim panel. Refer to Rear Side Door Sill Plate Replacement.

Important: When removing the trim take care not to damage the locating pins.

4. Carefully disengage the retaining trim clips (1) and remove the trim (2).

### Installation Procedure

Important: When installing the lower quarter trim panel, ensure the retaining clips are correctly aligned with the retainers before installation.

1. Carefully install the lower quarter trim panel (2) by engaging the retaining clips (1).
2. Install the rear sill trim panel. Refer to Rear Side Door Sill Plate Replacement.
3. Install the seat back assembly. Refer to Rear Seat Back Replacement.
4. Install the seat cushion. Refer to Rear Seat Cushion Replacement.