For 1990-2009 cars

## Propeller Shaft Transmission Flange Installation 6L50

Callout | Component Name
--- | ---
1 | Prop Shaft Trans Flange
2 | NEW Front Prop Shaft Flange Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 105 N·m (77 lb ft).

#### Special Tool

J 45012 Holding Fixture

For equivalent regional tools, refer to Special Tools.

3 | Output Shaft Caution: Stake the flange nut onto the output shaft. Use the two staking grooves on the shaft to locate the staking points. Failure to stake the flange nut may result in damage to the transmission.