For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Transmission Fluid Filler Tube Plug Tip

1. Clean the area around the filler tube plug before removal.
2. Use a door trim tool to release the filler tube plug interlock.