For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the camshaft position (CMP) actuator valve electrical connector (1) from the CMP (2).
3. Remove the CMP actuator solenoid valve to engine front cover retaining bolt (1).
4. Remove the CMP actuator valve (2).
5. Inspect the CMP actuator valve seal and replace as necessary.

### Installation Procedure

1. Inspect the CMP actuator valve seal for damage. Replace the seal if necessary.
2. Install the CMP actuator valve (2) to the engine front cover.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the CMP actuator solenoid valve to engine front cover retaining bolt (1).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the CMP valve electrical connector (1) to the CMP actuator valve.