For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the glove box assembly. Refer to Instrument Panel Compartment Replacement .
2. Remove the floor air outlet duct to instrument panel (I/P) retaining screws (1).
3. Remove floor air outlet duct (2) from the I/P.

### Installation Procedure

1. Install the floor air outlet duct 2 to the instrument panel (I/P).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the floor air outlet duct to I/P retaining screws (1) .

Tighten
Tighten the screws to 2 N·m(18lb in).

3. Install the glove box assembly. Refer to Instrument Panel Compartment Replacement .