For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result. Important: Clean and inspect all components and machined surfaces.
1 | Pressure Regulator Valve Train
2 | Converter Feed Limit Valve Train
3 | Pressure Relief Ball Valve and Spring
4 | TCC Control Valve and Spring
5 | 1-2-3-4 and 3-5 Reverse Clutch Fluid Seal Rings (Quantity: 3) Important: Discard the seal rings and replace with NEW rings.
6 | A/Trans Fluid Pump Locator Pin