For 1990-2009 cars

Important: Only remove the bolts called out in the graphic, there will be two remaining.

1. Remove the control valve body retaining bolts (49 and 51).
2. Remove the control valve body retaining bolts (53).
3. Remove the manual shaft detent (52).
4. Remove the control valve body (47).
5. Remove the centre support fluid passage sleeve (38) and the overdrive clutch fluid passage sleeve (39).