For 1990-2009 cars

## Torque Converter Housing with Fluid Pump Installation 6L50

Callout | Component Name
--- | ---
1 | NEW Fluid Pump Seal
2 | Torque Converter (with Fluid Pump) Housing Assembly Caution: Ensure the turbine shaft (O-ring) seal is not installed prior to installing the torque converter housing assembly. The seal may become cut or damaged during installation of the torque converter housing assembly.
3 | Bolts M8 x 1.25 x 50 (Qty: 8) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Tighten in sequence shown.

Tighten
31 N·m (23 lb ft)

4 | NEW Turbine Shaft (O-Ring) Seal