For 1990-2009 cars

### Removal Procedure (Type A)

1. Remove the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the secondary information centre. Refer to Secondary Driver Information Display Replacement .
3. Remove the I/P center air outlet deflector to I/P upper trim panel retaining screws (3).
4. Remove the I/P center air outlet deflector (2) from the I/P upper trim panel (1).

### Installation Procedure (Type A)

1. Install the I/P center air outlet deflector (2) to the I/P upper trim panel (1).
2. Install the I/P center air outlet deflector to I/P upper trim panel retaining screws (3).

Tighten
Tighten the screws to 2 N·m (18 lb in.)

3. Install the secondary information centre. Refer to Secondary Driver Information Display Replacement .
4. Install the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .

### Removal Procedure (Type B)

1. Remove the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the secondary information centre. Refer to Secondary Driver Information Display Replacement .
3. Remove the I/P center air outlet deflector to I/P upper trim panel retaining screws (3).
4. Remove the I/P center air outlet deflector (1) from the I/P upper trim panel (2).

### Installation Procedure (Type B)

1. Install the I/P center air outlet deflector (1) to the I/P upper trim panel (2).
2. Install the I/P center air outlet deflector to I/P upper trim panel retaining screws (3).

Tighten
Tighten the screws to 2 N·m (18 lb in.)

3. Install the secondary information centre. Refer to Secondary Driver Information Display Replacement .
4. Install the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .

### Removal Procedure (Type C)

1. Remove the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the I/P center air outlet deflector to I/P upper trim panel retaining screws (3).
3. Remove the I/P center air outlet deflector (2) from the I/P upper trim panel (1).

### Installation Procedure (Type C)

1. Install the I/P center air outlet deflector (2) to the I/P upper trim panel (1).
2. Install the I/P center air outlet deflector to I/P upper trim panel retaining screws (3).

Tighten
Tighten the screws to 2 N·m (18 lb in.)

3. Install the I/P upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .

### Removal Procedure (Type D)

1. Remove the console centre trim plate. Refer to Console Trim Plate Replacement .
2. Remove the instrument panel centre trim plate. Refer to Instrument Panel Center Trim Panel Replacement .
3. Remove the infotainment unit. Refer to Radio Replacement .

Important: Depress the I/P center air outlet deflector to I/P upper trim pad retaining clips (3) to disengage the I/P center air outlet deflector (1) from the I/P upper trim pad (2).

4. Disengage the I/P center air outlet deflector to I/P upper trim pad retaining clips (3).
5. Remove the I/P center air outlet deflector (1) from the I/P upper trim pad (2).

### Installation Procedure (Type D)

Important: Make sure the I/P center air outlet deflector to I/P upper trim pad retaining clips (3) are engaged to avoid an induced rattle condition.

1. Install the I/P center air outlet deflector (1) to the I/P upper trim pad (2).
2. Install the infotainment unit. Refer to Radio Replacement .
3. Install the instrument panel centre trim plate. Refer to Instrument Panel Center Trim Panel Replacement .
4. Install the console centre trim plate. Refer to Console Trim Plate Replacement .