For 1990-2009 cars

Table 1: | Accelerator Pedal Position (APP) Sensor (LY7/L98)
Table 2: | Backup Lamp Switch (LY7)
Table 3: | Camshaft Position (CMP) Exhaust Sensor - 1 (LY7)
Table 4: | Camshaft Position (CMP) Exhaust Sensor - 2 (LY7)
Table 5: | Camshaft Position (CMP) Exhaust Solenoid - 1 (LY7)
Table 6: | Camshaft Position (CMP) Exhaust Solenoid - 2 (LY7)
Table 7: | Camshaft Position (CMP) Intake Sensor - 1 (LY7)
Table 8: | Camshaft Position (CMP) Intake Sensor - 2 (LY7)
Table 9: | Camshaft Position (CMP) Intake Solenoid - 1
Table 10: | Camshaft Position (CMP) Intake Solenoid - 2
Table 11: | Clutch Cruise Switch
Table 12: | Clutch Safety Switch
Table 13: | Crankshaft Position (CKP) Sensor
Table 14: | Engine Coolant Temperature (ECT) Sensor (LY7)
Table 15: | Engine Oil Level/Temperature Sensor (LY7)
Table 16: | Engine Oil Pressure (EOP) Sensor (LY7)
Table 17: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LY7)
Table 18: | Fuel Injector - 1 (LY7)
Table 19: | Fuel Injector - 2 (LY7)
Table 20: | Fuel Injector - 3 (LY7)
Table 21: | Fuel Injector - 4 (LY7)
Table 22: | Fuel Injector - 5 (LY7)
Table 23: | Fuel Injector - 6 (LY7)
Table 24: | Fuel Level Sensor - Secondary
Table 25: | Fuel Pump and Sender Assembly
Table 26: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LY7)
Table 27: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LY7)
Table 28: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LY7)
Table 29: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LY7)
Table 30: | Ignition Coil - 1 (LY7)
Table 31: | Ignition Coil - 2 (LY7)
Table 32: | Ignition Coil - 3 (LY7)
Table 33: | Ignition Coil - 4 (LY7)
Table 34: | Ignition Coil - 5 (LY7)
Table 35: | Ignition Coil - 6 (LY7)
Table 36: | Knock Sensor (KS) Bank 1 (LY7)
Table 37: | Knock Sensor (KS) Bank 2 (LY7)
Table 38: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LY7/L98)
Table 39: | Throttle Body (LY7)
Table 40: | Variable Intake Manifold (VIM) Module
Table 41: | Variable Intake Manifold (VIM) Solenoid

#### Accelerator Pedal Position (APP) Sensor (LY7/L98)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN/YE | 0.5 | 5-Volt Reference
2 | WH/BK | 0.5 | 5-Volt Reference
3 | BU/WH | 0.5 | APP Sensor 1 Signal
4 | BN | 0.5 | Low Reference
5 | PU | 0.5 | Low Reference
6 | L-BU | 0.5 | APP Sensor 2 Signal

#### Backup Lamp Switch (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | L-GN | 0.5 | Backup Lamp Switch Signal
2 | BK | 0.5 | Ground

#### Camshaft Position (CMP) Exhaust Sensor - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BK | 0.75 | Low Reference
2 | D-GN | 0.5 | CMP Sensor Signal - Exhaust Bank 1
3 | GY | 0.75 | 5-Volt Reference

#### Camshaft Position (CMP) Exhaust Sensor - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BK | 0.5 | Low Reference
2 | PU | 0.5 | CMP Sensor Signal - Exhaust Bank 2
3 | GY | 0.5 | 5-Volt Reference

#### Camshaft Position (CMP) Exhaust Solenoid - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BU | 0.75 | Ignition 1 Voltage
2 | L-GN | 0.75 | CMP Actuator Solenoid Control - Exhaust Bank 1

#### Camshaft Position (CMP) Exhaust Solenoid - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BU | 0.75 | Ignition 1 Voltage
2 | WH/BK | 0.75 | CMP Actuator Solenoid Control - Exhaust Bank 2

#### Camshaft Position (CMP) Intake Sensor - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BK | 0.5 | Low Reference
2 | OG/BU | 0.5 | CMP Sensor Signal - Intake Bank 1
3 | GY | 0.5 | 5-Volt Reference

#### Camshaft Position (CMP) Intake Sensor - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BK | 0.5 | Low Reference
2 | PU | 0.5 | CMP Sensor Signal - Intake Bank 2
3 | GY | 0.5 | 5-Volt Reference

#### Camshaft Position (CMP) Intake Solenoid - 1

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BU | 0.75 | Ignition 1 Voltage
2 | PU | 0.75 | CMP Actuator Solenoid Control - Intake Bank 1

#### Camshaft Position (CMP) Intake Solenoid - 2

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BU | 0.75 | Ignition 1 Voltage
2 | OG/BK | 0.75 | CMP Actuator Solenoid Control - Intake Bank 2

#### Clutch Cruise Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN/WH | 0.5 | Cruise Cancel Signal
B | PK/BU | 0.5 | Ignition 1 Voltage

#### Clutch Safety Switch

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | OG/BK | 0.5 | Park/Neutral Signal
B | BK | 0.5 | Ground

#### Crankshaft Position (CKP) Sensor

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PU | 0.5 | Low Reference
2 | YE/BU | 0.5 | CKP Sensor Signal
3 | PU/WH | 0.5 | 5-Volt Reference

#### Engine Coolant Temperature (ECT) Sensor (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | YE/GN | 0.5 | ECT Sensor Signal
2 | BK | 0.5 | Low Reference

#### Engine Oil Level/Temperature Sensor (LY7)

Connector Part Information | GT 150 Sealed 4.5
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN | 0.5 | Oil Level Switch Signal
B | GN/YE | 0.5 | Oil Temperature Sensor Signal
C | BK | 0.5 | Low Reference

#### Engine Oil Pressure (EOP) Sensor (LY7)

Connector Part Information | GT 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN/RD | 0.5 | Low Reference
2 | GY | 0.5 | 5-Volt Reference
3 | BN/WH | 0.5 | Oil Pressure Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/BU | 0.75 | Ignition 1 Voltage
2 | D-GN/WH | 0.75 | EVAP Canister Purge Solenoid Control

#### Fuel Injector - 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.8 | Ignition 1 Voltage
B | BN/BK | 0.8 | Fuel Injector 1 Control

#### Fuel Injector - 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.8 | Ignition 1 Voltage
B | L-GN/BK | 0.8 | Fuel Injector 2 Control

#### Fuel Injector - 3 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.8 | Ignition 1 Voltage
B | PK/BK | 0.8 | Fuel Injector 3 Control

#### Fuel Injector - 4 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.8 | Ignition 1 Voltage
B | L-BU/BK | 0.8 | Fuel Injector 4 Control

#### Fuel Injector - 5 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.8 | Ignition 1 Voltage
B | BN/WH | 0.8 | Fuel Injector 5 Control

#### Fuel Injector - 6 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK | 0.8 | Ignition 1 Voltage
B | YE/BK | 0.8 | Fuel Injector 6 Control

#### Fuel Level Sensor - Secondary

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | BN/YE | 0.3 | Fuel Return
2 | L-BU | 0.5 | Fuel Level
3 | -- | -- | Not Used
4 | -- | -- | Not Used
5 | -- | -- | Not Used

#### Fuel Pump and Sender Assembly

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | GY | 2.0 | Fuel Pump Supply Voltage
2 | PU | 0.5 | Fuel Level Sensor Signal (Primary)
3 | BK | 2.0 | Ground
4 | BN/YE | 0.5 | Low Reference
5 | -- | -- | Not Used

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | WH | 0.5 | HO2S Output Pump Current (Bank 1 Sensor 1)
2 | BN/YE | 0.5 | HO2S Low Signal (Bank 1 Sensor 1)
3 | GY/WH | 0.75 | HO2S Heater Low Control (Bank 1 Sensor 1)
4 | PK/BUK | 0.75 | Ignition 1 Voltage
5 | L-GN | 0.5 | HO2S Input Pump Current (Bank 1 Sensor 1)
6 | PU/WH | 0.5 | HO2S High Signal (Bank 1 Sensor 1)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/D-BU | 0.75 | Ignition 1 Voltage
2 | OG/WH | 0.75 | HO2S Heater Low Control (Bank 1 Sensor 2)
3 | BN/RD | 0.5 | HO2S Low Signal (Bank 1 Sensor 2)
4 | PU | 0.5 | HO2S High Signal (Bank 1 Sensor 2)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PU/WH | 0.5 | HO2S Pump Output Current (Bank 2 Sensor 1)
2 | BN/RD | 0.5 | HO2S Low Signal (Bank 2 Sensor 1)
3 | L-GN | 0.75 | HO2S Heater Low Control (Bank 2 Sensor 1)
4 | PK/BU | 0.75 | Battery 1 Voltage
5 | OG | 0.5 | HO2S Input Pump Current (Bank 2 Sensor 1)
6 | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 1)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PK/D-BU | 0.75 | Battery 1 Voltage
2 | GY/WH | 0.75 | HO2S Heater Low Control (Bank 2 Sensor 2)
3 | BN/GN | 0.5 | HO2S Low Signal (Bank 2 Sensor 2)
4 | PU | 0.5 | HO2S High Signal (Bank 2 Sensor 2)

#### Ignition Coil - 1 (LY7)

Connector Part Information | Global Terminal/150
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.75 | Ground
B | PU | 0.5 | Low Reference
C | PU | 0.5 | IC 1 Control
D | PK/BU | 0.75 | Ignition 1 Voltage

#### Ignition Coil - 2 (LY7)

Connector Part Information | Global Terminal/150
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.75 | Ground
B | PK | 0.5 | Low Reference
C | OG/WH | 0.5 | IC 2 Control
D | PK | 0.75 | Ignition 1 Voltage

#### Ignition Coil - 3 (LY7)

Connector Part Information | Global Terminal/150
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.75 | Ground
B | PU | 0.5 | Low Reference
C | L-BU | 0.5 | IC 3 Control
D | PK/BU | 0.75 | Ignition 1 Voltage

#### Ignition Coil - 4 (LY7)

Connector Part Information | Global Terminal/150
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.75 | Ground
B | PK | 0.5 | Low Reference
C | D-GN/WH | 0.5 | IC 4 Control
D | PK | 0.75 | Ignition 1 Voltage

#### Ignition Coil - 5 (LY7)

Connector Part Information | Global Terminal/150
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.75 | Ground
B | PU | 0.5 | Low Reference
C | GN/RD | 0.5 | IC 5 Control
D | PK/BU | 0.75 | Ignition 1 Voltage

#### Ignition Coil - 6 (LY7)

Connector Part Information | Global Terminal/150
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BK | 0.75 | Ground
B | PK | 0.5 | Low Reference
C | L-BU/WH | 0.5 | IC 6 Control
D | PK | 0.75 | Ignition 1 Voltage

#### Knock Sensor (KS) Bank 1 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | D-BU | 0.5 | Knock Sensor 1 Signal
2 | GY | 0.5 | Low Reference Knock Sensor Signal Return

#### Knock Sensor (KS) Bank 2 (LY7)

Connector Part Information |
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | L-BU | 0.5 | Knock Sensor 2 Signal
2 | BN | 0.5 | Low Reference Knock Sensor Signal Return

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LY7/L98)

Connector Part Information | GT 150 Sealed 4.0
--- | ---
Pin | Wire Colour | Wire Size | Function
A | YE | 0.5 | MAF Sensor Signal
B | PK | 0.5 | Ignition 1 Voltage
C | BK | 0.5 | Ground
D | BN/RD | 0.5 | IAT Sensor Signal
E | BN/WH | 0.5 | Low Reference

#### Throttle Body (LY7)

Connector Part Information | GT 150 Series, Sealed
--- | ---
Pin | Wire Colour | Wire Size | Function
A | BN | 0.75 | TAC Motor Control - 2
B | YE | 0.75 | TAC Motor Control - 1
C | BN/BK | 0.5 | Low Reference
D | D-GN | 0.5 | TP Sensor 1 Signal
E | GY | 0.5 | 5-Volt Reference
F | PU | 0.5 | TP Sensor 2 Signal

#### Variable Intake Manifold (VIM) Module

Connector Part Information | GT 150 Sealed 4.0
--- | ---
Pin | Wire Colour | Wire Size | Function
A | PK/BU | 0.75 | Ignition 1 Voltage
B | BN | 0.75 | PWM_OUT
C | PU/BK | 0.75 | PWR_RTN
D | L-BU/WH | 0.75 | PWM
E | BK | 0.75 | Ground

#### Variable Intake Manifold (VIM) Solenoid

Connector Part Information | .090 Class II Sealed Series
--- | ---
Pin | Wire Colour | Wire Size | Function
1 | PU/BK | 0.75 | PWM_RTN
2 | BN | 0.75 | PWR_OUT