For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: Refer to Exhaust Service Caution in the Preface section.

2. Remove the left rear muffler assembly. Refer to Exhaust Muffler Replacement - Left Side.
3. Remove the left exhaust muffler heat shield to body retaining bolts (2).
4. Remove the left exhaust muffler heat shield (1).

### Installation Procedure

1. Position the left exhaust muffler heat shield (1) to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the left exhaust muffler heat shield to body retaining bolts (2).

Tighten
Tighten the bolts to 4 N·m (35 lb in).

3. Install the left rear muffler assembly. Refer to Exhaust Muffler Replacement - Left Side.
4. Lower the vehicle to the ground.