For 1990-2009 cars

### Removal Procedure

1. Remove the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement.
2. Remove the front sill trim plate. Refer to Front Side Door Sill Plate Replacement.
3. Remove the rear sill trim plate. Refer to Rear Side Door Sill Plate Replacement.
4. Remove the centre trim panel torx screw (1).

Important: When removing the centre sill trim panel, ensure the two white retaining clips at the top of the part remain in the sheet metal.

5. Remove the centre sill trim panel (1).

### Installation Procedure

Important: Before installing trims, ensure all retaining clips are not damaged, if damaged replace as necessary.

1. Install the centre sill trim panel.
2. Install the centre sill trim panel torx screw

Tighten
Tighten the centre sill trim panel torx screw (1) to 2.0 N·m (18 lb in).

3. Install the rear sill trim plate. Refer to Rear Side Door Sill Plate Replacement.
4. Install the front sill trim plate. Refer to Front Side Door Sill Plate Replacement.
5. Install the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement.