For 1990-2009 cars

Application | Specification
Metric | English
Propeller Shaft Rubber Coupling to Propeller Shaft Retaining Bolts and Nuts. | 20 N-m +55° | 15 lb ft +55°
Centre Bearing to Body Retaining Bolts. | 22 N-m | 16 lb ft
Propeller Shaft Rubber Coupling to Propeller Shaft Yoke Retaining Bolts and Nuts. | 20 N-m +55° | 15 lb ft +55°
Propeller Shaft Coupling to Differential Flange Retaining Bolts. | 115 N-m | 85 lb ft
Propeller Shaft Rubber Coupling to Transmission Flange Retaining Bolts and Nuts (torque bolt, hold nut). | 100 N-m | 72 lb ft