For 1990-2009 cars

### Removal procedure

1. Remove the driver side instrument panel lower trim. Refer to Instrument Panel Insulator Panel Replacement - Right Side.
2. Remove the aspirator tube (2) from the rear of the inside air temperature sensor (1).
3. Disconnect the inside air temperature sensor electrical connector (3).

Important: From the front of the inside air temperature sensor (3) use a suitable tool to push down on the four inside air temperature sensor to instrument panel carrier retaining clips (1). Withdraw the inside air temperature sensor (1) rearwards towards the bulkhead from the instrument panel carrier (3) .

4. Remove the inside air temperature sensor (3) from the instrument panel carrier (2).

### Installation Procedure

Important: Make sure the inside air temperature sensor to instrument panel carrier retaining clips (1) are correctly engaged to avoid an induced rattle condition.

1. Install the inside air temperature sensor (3) to the instrument panel carrier (2).
2. Connect the inside air temperature sensor electrical connector (3).
3. Install the aspirator tube (2) to the rear of the inside air temperature sensor (1).
4. Install the driver side instrument panel lower trim cover. Refer to Instrument Panel Insulator Panel Replacement - Right Side.