For 1990-2009 cars

### Removal Procedure

1. Remove the radiator air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement.
2. Remove the washer solvent container filler neck (4) to front end module bracket retaining bolt (2) and nut (1).
3. Remove the washer solvent container filler neck (4) to front end module bracket retaining torx screw (3).
4. Remove the washer solvent container filler neck (4) from the washer solvent container.

### Installation Procedure

1. Install the washer solvent container filler neck (4) into the washer solvent container.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the washer solvent container filler neck (4) to front end module bracket retaining bolt (2) and nut (1).

Tighten
Tighten the washer solvent container filler neck retaining bolt to 5.0 N·m (44 lb in).

3. Install the washer solvent container filler neck (4) to front end module bracket retaining torx screw (3).

Tighten
Tighten the retaining torx screw to (4.0 N·m (35 lb in).

4. Install the radiator air baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement.