For 1990-2009 cars

### Removal Procedure

1. Carefully unhook the convenience net (1) from the two lower retainer hooks (3) and the two upper retainer hooks (2).
2. Remove the convenience net from the rear compartment trim assembly.
3. If required, unscrew the two upper and two lower retainer hooks.

### Installation Procedure

1. If removed install the upper and lower retainer hooks (2 and 3).
2. Install the convenience (1) net to the rear compartment end panel.