For 1990-2009 cars

### Removal Procedure

1. Remove the cooling fan and shroud assembly. Refer to Cooling Fan and Shroud Replacement.

Important: Armature shaft and nut is left hand thread.

2. Remove the cooling fans (2) retaining nuts (3).
3. Remove the cooling fans (2) from the cooling fan motor (1).

### Installation Procedure

Important: When installing the cooling fans, ensure they are install as per removal.

1. Install the cooling fans (2) to the cooling fan motor (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cooling fan (2) to fan motor retaining nut (3).

Tighten
Tighten the nut to 6.0 N·m (53 lb in).

3. Install the cooling fan and shroud assembly. Refer to Cooling Fan and Shroud Replacement.
4. Start and run engine until cooling fans are activated.