For 1990-2009 cars

## Engine Flywheel Removal Automatic Transmission

#### Tools Required

EN 46106 Flywheel Holding Tool

1. Install the EN 46106 (1) through the starter mounting hole.

Important: Bolts with micro-encapsulated thread sealant must be discarded after removal.

Important: Make sure all the bolt holes are thoroughly cleaned and all micro-encapsulated thread sealant is removed.

2. Remove the engine flywheel to crankshaft retaining bolts (1).

• | Discard the bolts.

• | Clean the bolt holes.

3. Remove the engine flywheel (2).