For 1990-2009 cars

## Generator Bracket Replacement 3.6L Engine

### Removal Procedure

1. Remove the alternator. Refer to Generator Replacement.
2. Remove the coolant inlet pipe to alternator mounting bracket retaining nut (3).
3. Remove the alternator mounting bracket to cylinder block retaining bolts (4).
4. Remove the alternator mounting bracket (2) from the cylinder block (1).

### Installation Procedure

1. Install the alternator bracket (2) to the engine block.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the alternator bracket to engine block retaining bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Install the coolant inlet pipe to alternator mounting bracket retaining nut (3).

Tighten
Tighten the bolts to 22 N·m (16 lb ft).