For 1990-2009 cars

### Removal Procedure - Front

1. Remove the front door upper auxiliary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement.
2. Detach the door frame garnish molding locking tab (1) from the door frame (2) using a suitable flat bladed tool.
3. Remove the door frame garnish molding (1) from the door (2).

### Installation Procedure - Front

1. Position the door frame garnish molding (1) to the door (2).

Important: Push the door frame garnish molding until the locking tab (1) locates in the door frame (2).

2. Attach the door frame garnish molding locking tab (1) from the door frame (2).
3. Install the front door upper auxiliary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement.

### Removal Procedure - Rear

1. Remove the rear door bottom auxiliary weatherstrip. Refer to Rear Side Door Bottom Auxiliary Sealing Strip Replacement.
2. Detach the door frame garnish molding locking tab (1) from the door frame (2) using a suitable flat bladed tool.

Important: Detach the clips on the door frame garnish molding (1) with a suitable flat bladed tool.

3. Remove the door frame garnish molding (1) from the door (2).

### Installation Procedure - Rear

1. Install the door frame garnish molding (1) to the door (2).

Important: Push the door frame garnish molding until the locking tab (1) locates in the door frame (2).

2. Attach the door frame garnish molding locking tab (1) from the door frame (2).
3. Install the rear door bottom auxiliary weatherstrip. Refer to Rear Side Door Bottom Auxiliary Sealing Strip Replacement.