For 1990-2009 cars

### Removal Procedure

Important: When a suitable hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Install a suitable hood brace to the vehicle.
2. Remove the hood assist rod. Refer to Hood Open Assist Rod Replacement.
3. Remove the hood assist rod upper ball stud (1) from the hood.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the hood assist rod upper ball stud (1) to the hood.

Tighten
Tighten the ball stud to 18 N·m (15 lb ft).

2. Install the hood assist rod. Refer to Hood Open Assist Rod Replacement.
3. Remove the suitable hood brace from the vehicle.