For 1990-2009 cars

## Cigar Lighter Receptacle or 12-Volt Accessory Power Receptacle Replacement LWBLHD

### Instrument Panel

#### Tools Required

J 42059 Cigar Lighter Socket Remover

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. With any accessories removed, place the T receptacle of J 42059 into one of the retaining tabs (1). Angle the other side into the opposite retaining tab. Pull the power accessory receptacle straight out.
3. Disconnect the power accessory receptacle electrical connector (1).
4. Remove the bezel (1).

### Installation Procedure

1. Install the bezel (1).
2. Connect the power accessory receptacle electrical connector (1).
3. Install the accessory power receptacle to the receptacle bezel.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

### Centre Console -- Rear

#### Tools Required

J 42059 J 42059 Cigar Lighter Socket Remover

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. With any accessories removed, place the T receptacle of J 42059 into one of the retaining tabs (1). Angle the other side into the opposite retaining tab. Pull the power accessory receptacle straight out.
3. Disconnect the power accessory receptacle electrical connector (1).
4. Remove the bezel (1).

### Installation Procedure

1. Install the bezel (1).
2. Connect the power accessory receptacle electrical connector (1).
3. Install the accessory power receptacle to the receptacle bezel.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

### Centre Console

#### Tools Required

J 42059 Cigar Lighter Socket Remover

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Place the T receptacle of J 42059 into one of the retaining tabs (1). Angle the other side into the opposite retaining tab. Pull the power accessory receptacle straight out.
3. Disconnect the power accessory receptacle electrical connector (1).
4. Remove the bezel (1) and the cover (2).

### Installation Procedure

1. Install the cover (2) and the bezel (1).
2. Connect the power accessory receptacle electrical connector (1).
3. Install the accessory power receptacle to the receptacle bezel.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

### Rear Compartment

#### Tools Required

J 42059 Cigar Lighter Socket Remover

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Place the T receptacle of J 42059 into one of the retaining tabs (1). Angle the other side into the opposite retaining tab. Pull the power accessory receptacle straight out.
3. Disconnect the power accessory receptacle electrical connector (1).
4. Remove the cover (1) and the bezel(2).

### Installation Procedure

1. Install the cover (2) and the bezel (1).
2. Connect the power accessory receptacle electrical connector (1).
3. Install the accessory power receptacle to the receptacle bezel.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.