For 1990-2009 cars

## Front Seat Head Restraint Cover Replacement LWB

### Removal Procedure - WM Caprice with RSE

1. Remove the front seat head restraint. Refer to Front Seat Head Restraint Replacement .
2. Remove the rear entertainment screen assembly. Refer to Video Display Replacement .
3. Disengage the two J-strips (1) attaching the head restraint cover to the head restraint frame.
4. Using an appropriate tool, prise the retaining strips (2 and 4) from the three locking tabs (3) within the head restraint frame recess.

Important: Beginning at the upper corner, fold the cover away from the head restraint pad.

5. Remove the head restraint cover (1) from the head restraint pad (2).
6. Remove the cover (1) from the head restraint frame (1).
7. Remove the pad (2) from the frame (1).

### Installation Procedure - WM Caprice with RSE

1. Install the pad (2) to the frame (1).
2. Install the cover (1) to the head restraint frame (1).

Important: Beginning at the lower corner, wrap the cover around the head restraint pad.

3. Install the head restraint cover (1) to the head restraint pad (2).
4. Insert the retaining strips (2 and 4) to the three locking tabs (3) within the head restraint frame recess.
5. Insert the two J-strips (1) attaching the head restraint cover to the head restraint frame.
6. Install the rear entertainment screen assembly. Refer to Video Display Replacement .
7. Install the front seat head restraint. Refer to Front Seat Head Restraint Replacement .
8. Upon completion inspect the head restraint and caress the trim cover to ensure it is seated properly and offers a high quality appearance.