For 1990-2009 cars

Table 1: | 2-6 Clutch Plates Removal
Table 2: | 2-6 Clutch Piston Replacement
Table 3: | 2-6 Clutch Plates Installation

### 2-6 Clutch Plates Removal

Callout | Component Name
--- | ---
1 | 2-6 Clutch Backing Plate Retaining Ring
2 | 2-6 Clutch Backing Plate
3 | 2-6 Clutch Plate Assembly (Quantity: 5)
4 | 2-6 Clutch Plate (Quantity: 5)
5 | 2-6 Clutch (Waved) Plate

### 2-6 Clutch Piston Replacement

Callout | Component Name
--- | ---
1 | 2-6 Clutch Spring Retaining Ring Tip Ensure the DT 47761 is centred over the clutch spring.

#### Special Tool

DT 47761

2 | 2-6 Clutch Spring Notice: Refer to General Repair Instructions in the Preface section.
3 | 2-6 Clutch Piston Assembly Tip It may be necessary to apply air to the apply passage in order to unseat the piston.

### 2-6 Clutch Plates Installation

Callout | Component Name
--- | ---
1 | 2-6 Clutch (Waved) Plate
2 | 2-6 Clutch Plates (Quantity: 5) Tip Alternate between steel and fibre clutch plates.
3 | 2-6 Clutch Plate Assembly (Quantity: 5) Tip Alternate between steel and fibre clutch plates.
4 | 2-6 Clutch Backing Plate
5 | 2-6 Clutch Backing Plate Retaining Ring
6 | 2-6 Clutch Apply Passage Tip Apply air to verify proper installation of all 2-6 clutch components.