For 1990-2009 cars

## Dimensions - Body LWB

Location | Description | Length | Width | Height
--- | --- | --- | --- | ---
1 | Zero Line 19 mm Gage Hole | 0 | 0 | 0
A | Door Hinge Attach | 76 mm (2.99 in) | 1687 mm (66.42 in) | 363 mm (14.29 in)
B | Door Hinge Attach | 155 mm (6.1 in) | 1592 mm (62.68 in) | 452 mm (17.8 in)
C | Door Hinge Attach | 1186 mm (46.69 in) | 1704 mm (67.09 in) | 757 mm (29.8 in)
D | Upper Door Lock Striker Attach | 1173 mm (46.18 in) | 1633 mm (64.29 in) | 621 mm (24.45 in)
E | Door Hinge Attach | 1166 mm (45.91 in) | 1701 mm (66.97 in) | 461 mm (18.15 in)
F | Upper Door Lock Striker Attach | 2225 mm (87.6 in) | 1640 mm (64.57 in) | 793 mm (31.22 in)
All dimensions are measured from a zero line, a center line, and a common datum. All dimensions are symmetrical unless otherwise specified.

### Point-to-Point Measurements

Location | Description | Length
--- | --- | ---
A | Lower Top Front Door Hinge Hole to Lower Top Rear Door Hinge Hole | 1103 mm (43.43 in)
B | Hinge Pillar Datum Hole to Lower Top Rear Door Hinge Hole | 1205 mm (47.44 in)
C | Hinge Pillar Datum Hole to Lower Bottom Rear Door Hinge Hole | 1170 mm (46.06 in)
D | Lower Bottom Front Door Hinge Hole to Lower Bottom Rear Door Hinge Hole | 1086 mm (42.76 in)
E | Lower Top Rear Door Hinge Hole to Upper Rear Door Striker Hole | 1042 mm (41.02 in)
F | Lower Top Rear Door Hinge Hole to Lower Body Side Datum Hole | 957 mm (37.68 in)
G | Lower Bottom Front Door Hinge Hole to Lower Body Side Datum Hole | 853 mm (33.58 in)
H | Lower Body Side Datum Hole to Rear Body Side Datum Hole | 958 mm (37.72 in)
All dimensions are measured from a zero line, a center line, and a common datum. All dimensions are symmetrical unless otherwise specified.

### Dimensions - Underbody

Location | Description | Length | Width | Height
--- | --- | --- | --- | ---
1 | Zero Line 18 mm Hole | 1535 mm (60.43 in) | 810 mm (31.89 in) | 128 mm (5.04 in)
A | 20 mm Hole | 1136 mm (44.72 in) | 0 | 0
B | 10 mm Bumper Mounting | 805 mm (31.69 in) | 886 mm (34.88 in) | 328 mm (12.91 in)
C | 16 mm Hole | 2234 mm (87.95 in) | 1024 mm (40.31 in) | 200 mm (7.87 in)
D | 25.1 mm x 39.7 mm Gage Hole | 3114 mm (122.6 in) | 1048 mm (41.26 in) | 434 mm (17.09 in)
E | 25.1 mm x 39.7 mm Gage Hole | 3318 mm (130.63 in) | 1048 mm (41.26 in) | 434 mm (17.09 in)
F | 18 mm Bumper Mounting | 3538 mm (139.29 in) | 0 | 0
All dimensions are measured from a zero line, a center line, and a common datum. All dimensions are symmetrical unless otherwise specified.