For 1990-2009 cars

### Removal Procedure

1. Remove seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the rear seat back. Refer to Rear Seat Back Replacement in Seats.
3. If fitted, remove head restraints. Refer to Rear Seat Head Restraint Replacement.
4. Place seat on suitable work surface.
5. Turn seat over on its front.
6. Detach the J-strips (1) retaining the back of the cover to the seat pad and frame.
7. While holding the seat back pad, remove the seat back cover.

### Installation Procedure

1. Align the aplix with the seat cover.
2. Install the seat cover.
3. Turn the seat back over on its front.

Important: When installing the seat cover, pull the cover tight in all corners to ensure no lumps will occur.

4. Attach the seat back cover J-strips to the seat back pad and frame.
5. If fitted, install head restraints. Refer to Rear Seat Head Restraint Replacement.
6. Install the rear seat back. Refer to Rear Seat Back Replacement in Seats.
7. Install seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement.