For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Brake Dust Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheels. Refer to Tire and Wheel Removal and Installation .
3. Disconnect the wheel speed sensor electrical connector (1).
4. Remove the wheel speed sensor to knuckle retaining bolt (3).
5. Remove the wheel speed sensor (2) from the knuckle (1).

### Installation Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Brake Dust Caution in the Preface section.

1. Install the wheel speed sensor (2) to the knuckle (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the wheel speed sensor to knuckle retaining bolt (3).

Tighten
Tighten the bolt to 7 Nm (62 lb in).

3. Connect the wheel speed sensor jumper harness electrical connector (1).
4. Install the rear wheels. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.