For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
3. Remove the front wheelhouse liner to the front air deflector push-in retainers (1).
4. Remove the front wheelhouse liner to rocker panel retaining screws (1).
5. Remove the front wheelhouse liner to wheelhouse retaining scrivets (1).
6. Remove the front wheelhouse liner from the vehicle.

### Installation Procedure

1. Position the front wheelhouse liner to the vehicle.
2. Install the front wheelhouse liner to wheelhouse retaining scrivets (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front wheelhouse liner to rocker panel retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the front wheelhouse liner to the front air deflector retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

5. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.