For 1990-2009 cars

### Removal Procedure (Up to 01 Jan 2008)

1. Open the front and rear door.

Caution: Refer to Safety Glasses Caution in the Preface section.

Important: Disengage the sill name plate(s) retaining clips (1), starting from either end of the sill name plate(s) (2).

Important: When removing the sill name plate(s), make sure the retaining clips (1) are retained in the sill name plate(s).

2. Using a suitable tool carefully remove the sill name plate(s) (2).

### Installation Procedure (Up to 01 Jan 2008)

Important: Before installing rear side door sill name plate(s) (2), make sure all retaining clips (1) are not damaged, if damaged replace as necessary.

Important: Make sure the lip of the weatherstrip sits over the sill plate.

1. Carefully align the rear side door sill name plate retaining clips (1) with the body locating holes.
2. Install the rear side door sill name plate(s), by firmly pushing down on the sill plate(s). Listen for an audible click to confirm fitting.

### Removal Procedure (From 01 Jan 2008)

1. Open the front and rear door.

Caution: Refer to Safety Glasses Caution in the Preface section.

Important: Disengage the sill name plate retaining clips (1), starting from either end of the sill name plate (2).

Important: When removing the side door sill name plate (2), make sure the retaining clips (1) are retained in the sill name plate.

2. Using a suitable tool carefully remove the sill name plate (2).

### Installation Procedure (From 01 Jan 2008)

Important: Before installing sill name plate (2), make sure all retaining clips (1) are not damaged, if damaged replace as necessary.

1. Carefully align the sill name plate retaining clips (1) with the body locating holes.

Important: Make sure the lip of the weatherstrip sits over the sill name plate (2).

2. Install the side door sill name plate (2), by firmly pushing down on the sill name plate. Listen for an audible click to confirm fitting.