For 1990-2009 cars

Application | Specification
--- | ---
| Metric | English
Battery Cable to Battery Terminal Retaining Nut | 17 N·m | 13 lb ft
Battery Negative Cable to Engine Block Retaining Bolt | 25 N·m | 18 lb ft
Battery Negative Cable to Engine Block Stud (LY7) | 25 N·m | 37 lb ft
Battery Positive Cable to Starter Terminal Retaining Nut (LY7, L98) | 13 N·m | 115 lb in
Battery Positive Cable to UBC Retaining Nut | 15 N·m | 11 lb ft
Battery Retainer Bolt | 18 N·m | 13 lb ft
Battery Tray to Chassis Retaining Bolt | 6 N·m | 53 lb in
Alternator to Block Retaining Bolt (Front) | 50 N·m | 37 lb ft
Alternator to Block Retaining Bolt (Side) | 50 N·m | 37 lb ft
Alternator Bracket to Block Retaining Bolt (Main) | 23 N·m | 17 lb ft
Alternator Output Battery Terminal Nut (V8) | 10 N·m | 89 lb in
Alternator Bracket to Block Retaining Bolts (alternator Support) | xx N·m | xx lb in
Alternator to Alternator Bracket Retaining Studs | xx N·m | xx lb in
Alternator to Alternator Bracket Retaining Nuts | xx N·m | xx lb in
Power Steering Pump to Power Steering Pump Bracket Retaining Bolts | xx N·m | xx lb in
Alternator Output Battery Terminal Nut (LY7) | 13 N·m | 115 lb in
Ground Strap to Cylinder Head Bolt (L98) | 25 N·m | 18 lb ft
Starter Motor Bolt (L98) | 30 N·m | 22 lb ft
Starter Motor Bolt (LY7) | 50 N·m | 37 lb ft
Starter Solenoid B+ Terminal Nut (L98, LY7) | 4 N·m | 35 lb in
Heatsheild to Starter Motor Retaining Bolts | xx N·m | xx lb in
Battery Cable to Battery Clamp Retaining Nut | 17 N·m | 13 lb ft
Battery Negative Cable to Chassis Retaining Bolt | 15 N·m | 11 lb ft
Battery Positive Cable to Alternator Battery Output Terminal Retaining Bolt | 4 N·m | 35 lb in
Battery Positive Cable to Battery Remote Positive Post Retaining Bolt | xx N·m | xx lb in
Battery Positive Cable to Alternator Battery Output Terminal Retaining Nut | xx N·m | xx lb in
Battery Positive Cable to Starter Motor Terminal Retaining Nut | 13 N·m | 115 lb in
Battery Retainer Plate to Battery Retainer Strap Retaining Nut | 18 N·m | 13 lb ft
Ground Strap to Chassis Retaining Bolt | xx N·m | xx lb in
Starter Motor to Cylinder Block Retaining Bolts - 3.6L | 58 N·m | 42 lb ft
Starter Motor to Bell Housing Retaining Bolts - 6.0L | xx N·m | xx lb in
Starter Motor Soleniod Cable to Starter Motor Retaining Bolts V6 | 20 N·m | 14 lb ft
Starter Motor Soleniod Cable to Starter Motor Retaining Bolts V8 | 10 N·m | 89 lb in