For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result. Notice: Refer to General Repair Instructions in the Preface section. Important: Clean and inspect all valve components, locating pins, and the valve body. The control valve upper body is replaceable only as an assembly.
1 | Clutch Boost Valve Train
2 | 1-2-3-4 Clutch Regulator Valve Train
3 | 3-5 Reverse Clutch Regulator Valve Train
4 | Clutch Boost Valve Train
5 | 2-6 Clutch Regulator Valve Train
6 | Clutch Boost Valve Train
7 | 1/Reverse Band and 4-5-6 Clutch Regulator Valve Train
8 | Actuator Feed Limit Valve Train
9 | Control Valve Body Locator Pin
10 | Control Valve Body Locator Pin
11 | Control Valve Body Locator Pin