For 1990-2009 cars

## Instrument Cluster Trim Panel Replacement LWB

### Removal Procedure

Important: Note original position of the steering wheel and column assembly with regards to steering wheel height and reach.

1. Release the steering column tilt lever.

Fully lower the steering wheel and column assembly.

2. Remove the instrument cluster trim panel to instrument panel retaining screws (1).
3. Depress the top of the instrument cluster trim panel slightly and tilt out of the instrument panel, disengaging the retaining clips (2) each side.
4. Disengage the retaining lugs (3) from the instrument panel.
5. Remove the instrument cluster trim panel.

### Installation Procedure

1. Install the instrument cluster trim panel.
2. Engage the retaining lugs (3) into the instrument panel.
3. Engage the instrument cluster trim panel retaining clips (2).
4. Install the instrument cluster trim panel to instrument panel retaining screws (1).