For 1990-2009 cars

### Removal Procedure

1. Lower the window to the full down position.

Important: Pull the rear door outer belt sealing strip (1) up to detach the retainers.

2. Remove the rear door outer belt sealing strip (1) from the rear door (2).

### Installation Procedure

Important: Push the rear door outer belt sealing strip (1) down to attach the retainers.

1. Install the rear door outer belt sealing strip (1) to the rear door (2).
2. Raise the rear door window.