For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
End Plate to Power Steering Pump Housing Retaining Bolts | 22 N·m | 16 lb ft
Front Castor Arm Ball Joint to Steering Knuckle Retaining Nut

- First Pass

40 N·m

30 lb

- Final Pass

60 degrees

High Pressure Outlet Fitting to Power Steering Pump Housing | 59 N·m | 44 lb ft
Intermediate Steering Shaft to Pinion Shaft Retaining Bolt | 25 N·m | 18 lb ft
Power Steering Fluid Reservoir Outlet Hose Worm Drive Clamp | 2 N·m | 18 lb in
Power Steering Fluid Reservoir Inlet Pipe/Hose Bracket to Subframe Retaining Bolt | 9 N·m | 80 lb in
Power Steering Gear Outlet Pipe/Hose Bracket to Subframe Retaining Bolt | 9 N·m | 80 lb in
Power Steering Gear Inlet Pipe/Hose to Power Steering Gear Retaining Banjo Bolt | 58 N·m | 43 lb ft
Power Steering Gear Inlet Pipe to Power Steering Pump Retaining Banjo Bolt | 48 N·m | 35 lb ft
Power Steering Gear Inlet Pipe/Hose Bracket to Subframe Retaining Bolt | 9 N·m | 80 lb in
Power Steering Gear Outlet Pipe/Hose to Power Steering Gear Retaining Banjo Bolt | 58 N·m | 43 lb ft
Power Steering Pump Inlet Pipe to Power Steering Pump Housing Retaining Bolt | 10 N·m | 89 lb in
Power Steering Pump to Power Steering Pump Bracket Retaining Bolts | 27 N·m | 20 lb ft
Steering Gear to Subframe Retaining Bolts | 65 N·m | 48 lb ft
Tie Rod End Retaining Lock Nut | 50 N·m | 37 lb ft
Tie Rod End to Steering Knuckle Retaining Nut
First Pass | 25 N·m | 18 lb ft
Final Pass | 120 degrees