For 1990-2009 cars

## Intake Manifold Installation LY7

1. Install the NEW intake manifold gasket.
2. Install the intake manifold (2) and the throttle body (3) as an assembly as an assembly.

Notice: Refer to Fastener Notice in the Preface section.

Important: Tighten the intake manifold bolts (1) in a circular pattern starting at the center (long bolts) and moving outward.

3. Install the intake manifold bolts (1).

Tighten
Tighten the intake manifold bolts to 23 N·m (17 lb ft).

4. Install the fuel injector harness electrical connector/EVAP valve mounting bracket (1).
5. Install the fuel injector harness electrical connector/EVAP valve mounting bracket to intake manifold retaining bolt (2).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

6. Attach the fuel injector harness electrical connector (3) to the fuel injector harness electrical connector/EVAP valve mounting bracket (1).
7. Connect the EVAP hose (1) to the upper intake manifold (2).
8. Install the PCV tube and PCV fresh air tubes. Refer to Positive Crankcase Ventilation Hose/Pipe/Tube Replacement.