For 1990-2009 cars

Checks | Causes
--- | ---
2-6 and 3-5-R Clutch Hub Thrust Bearing Assembly (65) | Inspect the bearing for wear or damage.
Output Carrier Assembly (68) |

• | Inspect the carrier assembly for damaged pinion gears, thrust washers, pins, and rollers.

• | Inspect for a damaged centre support roller bearing assembly (485).

• | Inspect for damaged thrust bearings (486, 488).

• | Inspect for damaged sun gears (487, 489).

• | Inspect the carrier assembly for damaged output carrier rear sun gear thrust bearing (captured).

• | Inspect for damaged or stripped splines on the output carrier assembly.

Output Carrier Thrust Bearing Assembly (69) | Inspect the bearing for wear or damage.
Output Shaft Assembly (70) |

• | Inspect for damaged internal gears (495, 497).

• | Inspect the output carrier bushing (498) for damage or wear.

Output Shaft Thrust Bearing Assembly (71) | Inspect the bearing for wear or damage.
Input Sun Gear Thrust Washer (55) | Inspect the washer for wear or damage.
Input Sun Gear Thrust Bearing (54) | Inspect the bearing for wear or damage.
Input Sun Gear (53) | Inspect for spline wear or damage.
Input Carrier Assembly (52) | Inspect the carrier assembly for damaged pinion gears, thrust washers, pins, and rollers.
1-2-3-4 Clutch Hub Thrust Bearing Assembly (63) | Inspect the bearing for wear or damage.
2-6 and 3-5-R Clutch (with Output Carrier Outer Sun Gear Shaft) Hub Assembly (64) | Inspect the output carrier inner sun gear shaft bushings (60 and 62) for damage or wear.
Turbine Shaft Thrust Bearing Assembly (57) | Inspect the bearing for wear or damage.
Fluid Filter Assembly (26) |

• | Inspect for damaged or restricted fluid filter assembly (26)

• | Inspect for damaged fluid filter seal assembly (25) or improper sealing interface (leaks, fluid aeration).

Automatic Transmission Fluid Pump Seal (5) | Inspect for worn or damaged seal.