For 1990-2009 cars

1. Remove the ignition coil to camshaft cover retaining bolts (1).
2. Remove the ignition coils (2) from the camshaft cover (3).
3. Remove the spark plugs (1).
4. Remove the camshaft cover to cylinder head retaining bolts (1).
5. Remove the camshaft cover (2) from the cylinder head (3).

Important: The camshaft cover seal and grommets must be discarded whenever the camshaft cover has been removed from the cylinder head (2).

6. Remove the camshaft cover seal and grommets.

Discard the seal and grommets