For 1990-2009 cars

## Auxiliary Temperature Valve Actuator Replacement LWB LHD

### Removal Procedure

1. Remove the Instrument Panel Centre Trim Panel. Refer to Instrument Panel Center Trim Panel Replacement.
2. Remove the left side rear floor duct. Refer to Floor Rear Air Outlet Duct Replacement - Left Side.
3. Locate the Mode Door Actuator - Auxiliary (3) on the HVAC module assembly.
4. Disconnect the electrical connector (1) from the Mode Door Actuator - Auxiliary.
5. Remove the Mode Door Actuator - Auxiliary actuator to HVAC module assembly retaining screws (2).

### Installation Procedure

1. Install the Mode Door Actuator - Auxiliary (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the Mode Door Actuator - Auxiliary to HVAC module assembly retaining screws (2).

Tighten
Tighten the bolts to 1.5 N·m (13 lb ft).

3. Install the electrical connector (1) to the Mode Door Actuator - Auxiliary.
4. Install the left side rear floor duct. Refer to Floor Rear Air Outlet Duct Replacement - Left Side.
5. Install the Instrument Panel Centre Trim Panel. Refer to Instrument Panel Center Trim Panel Replacement.
6. Perform HVAC system relearn.