For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the rivet (2) that secures the front bumper fascia reinforcement (1) to the front bumper fascia. The rivet must be discarded after removal.

Discard the rivet.

3. Remove the front bumper fascia reinforcement (1) from the front bumper fascia.

### Installation Procedure

1. Position the front bumper fascia reinforcement (1) to the front bumper fascia.
2. Install the NEW rivet (2) to secure the front bumper fascia reinforcement to the front bumper fascia.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .