For 1990-2009 cars

## Scan Tool Output Controls 0

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
ABS Motor Test | -- | Used in order to command the ABS pump motor On or Off.
Automated Bleed Procedure | -- | Used in order to bleed ABS hydraulics. Refer to Antilock Brake System Automated Bleed Procedure.
LF Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LF Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RF Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RF Outlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
RR Inlet Valve Solenoid | Solenoid Test | Commands the solenoid ON and OFF.