For 1990-2009 cars

## Air Inlet Assembly Replacement LHD

### Removal Procedure

1. Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the close out panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side or Instrument Panel Insulator Panel Replacement - Left Side.
3. Remove the upper air inlet assembly bolts (1).
4. Remove the lower right air inlet assembly bolt (1).
5. Slide the assembly to the right and then lower.
6. Disconnect the air inlet assembly electrical connector (1).
7. Rotate the air inlet assembly clockwise (1) and remove.

### Installation Procedure

1. Connect the air inlet assembly electrical connector (1).
2. Install the air inlet assembly (1) to the locator pin.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the upper air inlet assembly bolts (1).

Tighten
Tighten the bolt to 9 N·m (80 lb in).

4. Install the lower right air inlet assembly bolt (1).

Tighten
Tighten the bolt to 9 N·m (80 lb in).

5. Install the I/P compartment. Refer to Instrument Panel Compartment Replacement.
6. Install the closeout panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side or Instrument Panel Insulator Panel Replacement - Left Side.