For 1990-2009 cars

## Rear Bumper Fascia Extension Replacement SWBLWB

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheelhouse liner. Refer to Rear Inner Wheelhouse Replacement.
3. Remove the rear bumper fascia extension to rear bumper fascia retaining screw (1).
4. Disengage the rear bumper fascia extension retaining clips (1) from the rear bumper fascia.
5. Remove the rear bumper fascia extension (2) from the vehicle.

### Installation Procedure

1. Position the rear bumper fascia extension (2) to the vehicle.
2. Engage the rear bumper fascia extension retaining clips (1) to the rear bumper fascia.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear bumper fascia extension to rear bumper fascia retaining screw (1).

Tighten
Tighten the screw to 2 N·m (18 lb in).

4. Install the rear wheelhouse liner. Refer to Rear Inner Wheelhouse Replacement.
5. Lower the vehicle.